**ADDENDUM #001 TO THE REQUEST FOR PROPOSAL DOCUMENT**

To all Bidders of Record on the Request for Proposal (RFP) titled:

**REQUEST FOR QUALIFICATIONS & PROPOSALS- COMPETITIVE Bid Construction Services**

**NEW KINDERGARTEN CLASSROOMS CONSTRUCTION**

**AVENAL ELEMENTARY SCHOOL**

Addendum Date: Dec 1, 2020

1. **This Addendum shall be considered part of the Request for Proposal document for the above-mentioned project as though it had been issued at the same time and shall be incorporated integrally therewith. Where provisions of the following supplementary data differ from those of the original RFP document, this Addendum shall govern and take precedence.**
2. **Bidders are hereby notified that they shall make any necessary adjustments in their estimates as a result of this addendum. It will be construed that each bidder’s proposal is submitted with full knowledge of all modifications and supplemental data specified herein.**

The RFP document are modified and clarified, as follows:

**Item #1**

Changes to the RFP Document:

* Cover Page
  + Replace Text reads *“Bid opening Thursday* ***Dec 3, 2020, 2:00PM”***

Replacement text to *“Bid opening Tuesday* ***Dec 8, 2020, 2:00PM”***

* Section 00010 Notice to Contractors Calling for Bids:
  + Replace Text reads *“Bids Due by Thursday* ***Dec 3, 2020, 2:00PM”***

Replacement text to *“Bids Due by Tuesday* ***Dec 8, 2020, 2:00PM”***

* Refer to Project Manual on the link under 1.01.2

1.1.1         Insert the attached sections: 011000 SUMMARY OR WORK, 012100 ALLOWANCES, 012600 MODIFICATION PROCEDURES, 013000 PROJECT COORDINATION, 013100 PROJECT MEETINGS, 013300 SUBMITTALS, 014000 QUALITY CONTROL SERVICES, DSA 103-19: LISTING OF STRUCTURAL TESTS & SPECIAL INSPECTIONS, 014300 GOVERNING (REVIEWING AND APPROVING) AGENCY, 015000 TEMPORARY FACILITIES, 017700 PROJECT CLOSEOUT, 017800 WARRANTIES AND BONDS, 018000 CONSTRUCTION WASTE REDUCTION, DISPOSAL AND RECYCLING AND 018000 STORM WATER POLLUTION PREVENTION PLAN between Section 00800 and 024119.

1.2               Refer to Sheet A1.20, SITE PLAN KEYNOTES, Keynote ‘02’:

1.2.1         Revise “SYNTHETIC TURF” to “SYNTHETIC TURF – FURNISHED BY OWNER AND INSTALLED BY SUPPLIER – SEE DETAIL FOR CORDINATION REQUIREMENTS”

1.3               Refer to Sheet A1.20, SITE PLAN KEYNOTES, Keynote ‘10’:

1.3.1         Revise “30’-0” x 40’-0” SHADE STRUCTURE – SEE MFR PC SHTS” to “30’-0” x 40’-0” SHADE STRUCTURE – FURNISHED BY OWNER AND INSTALLED BY SUPPLIER– SEE MFR PC SHTS”

1.4               Refer to Sheet A8.01, Detail ‘55’:

1.4.1         Add:

“NOTE:

1. CHAIN LINK MESH TO HAVE VERTICAL BOTTOM LOCKING SLATS. SLATS TO BE HDPE SLATS W/ UV INHIBITOR (“RIDGED SLATS” OR EQUAL).”

End of Addendum #1

Attachments:

Request for Proposal for Architectural Services, Addendum #1 revisions incorporated.